Jump to main content

##

# TCPIP_DHCPV6_CLIENT_STATE Enumeration

## C

    typedef enum {
    TCPIP_DHCPV6_CLIENT_STATE_INIT = 0,
    TCPIP_DHCPV6_CLIENT_STATE_IDLE,
    TCPIP_DHCPV6_CLIENT_STATE_RUN,
    TCPIP_DHCPV6_CLIENT_STATE_WAIT_LINK,
    TCPIP_DHCPV6_CLIENT_STATE_NUMBER
    } TCPIP_DHCPV6_CLIENT_STATE;

## Description

Enumeration: TCPIP_DHCPV6_CLIENT_STATE.

This enumeration lists the current status of the DHCPv6 module. Used in getting info about the DHCPv6 state machine.

## Members

Members | Description
--- | ---
TCPIP_DHCPV6_CLIENT_STATE_INIT = 0 | Initialization state/unknown.
TCPIP_DHCPV6_CLIENT_STATE_IDLE | Idle/inactive state.
TCPIP_DHCPV6_CLIENT_STATE_RUN | Up and running in one of the run states.
TCPIP_DHCPV6_CLIENT_STATE_WAIT_LINK | Up and running, waiting for a connection.
TCPIP_DHCPV6_CLIENT_STATE_NUMBER | Number of states.