Jump to main content

##

# 1.2.5.9.3 Library Interface

Name | Description
--- | ---
Macros |
_DRV_MIIM_CONFIG_H | This is macro _DRV_MIIM_CONFIG_H.
_DRV_MIIM_H | This is macro _DRV_MIIM_H.
DRV_MIIM_CLIENT_OP_PROTECTION | Enables/Disables Client Operation Protection feature.
DRV_MIIM_COMMANDS | Enables/Disables MIIM commands feature.
DRV_MIIM_INDEX_0 | MIIM driver index definitions.
DRV_MIIM_INDEX_COUNT | Number of valid MIIM driver indices.
DRV_MIIM_INSTANCE_CLIENTS | Selects the maximum number of clients.
DRV_MIIM_INSTANCE_OPERATIONS | Selects the maximum number of simultaneous operations for an instance.
DRV_MIIM_INSTANCES_NUMBER | Selects the maximum number of hardware instances that can be supported by the dynamic driver.
Functions |
DRV_MIIM_ClientStatus | Gets the current client-specific status the MIIM driver.
DRV_MIIM_Close | Closes an opened instance of the MIIM driver.
DRV_MIIM_Deinitialize | Deinitializes the specified instance of the MIIM driver module.
DRV_MIIM_DeregisterCallback | Deregisters an notification callback function for the client operations.
DRV_MIIM_Initialize | Initializes the MIIM driver.
DRV_MIIM_Open | Opens the specified MIIM driver instance and returns a handle to it.
DRV_MIIM_OperationAbort | Aborts a current client operation initiated by the MIIM driver.
DRV_MIIM_OperationResult | Gets the result of a client operation initiated by the MIIM driver.
DRV_MIIM_Read | Initiates a SMI/MIIM read transaction.
DRV_MIIM_RegisterCallback | Registers an notification callback function for the client operations.
DRV_MIIM_Reinitialize | Reinitializes the driver and refreshes any associated hardware settings.
DRV_MIIM_Scan | Initiates a SMI/MIIM scan (periodic read)transaction.
DRV_MIIM_Setup | Sets up a MIIM client.
DRV_MIIM_Status | Provides the current status of the MIIM driver module.
DRV_MIIM_Tasks | Maintains the driver's state machine.
DRV_MIIM_Write | Initiates a SMI/MIIM write transaction.
Enumerations |
DRV_MIIM_CLIENT_STATUS | Defines the possible results of operations that can succeed or fail
DRV_MIIM_OPERATION_FLAGS | List of flags that apply to a client operation.
DRV_MIIM_SETUP_FLAGS | List of flags that apply to a client setup operation.
Structures |
DRV_MIIM_INIT | Contains all the data necessary to initialize the MIIM device.
DRV_MIIM_OBJECT_BASE | Declaration of a MIIM base object.
DRV_MIIM_SETUP | Contains all the data necessary to set up the MIIM device.
Types |
DRV_MIIM_CALLBACK_HANDLE | Handle that identifies a client registration operation.
DRV_MIIM_OPERATION_CALLBACK | Notification function that will be called when a MIIM operation is completed and the driver client needs to be notified.
DRV_MIIM_OPERATION_HANDLE | MIIM operation handle.
Variables |
DRV_MIIM_OBJECT_BASE_Default | The supported basic MIIM driver (DRV_MIIM_OBJECT_BASE). This object is implemented by default as using the standard MIIM interface. It can be overwritten dynamically when needed.