Jump to main content

##

# TCPIP_DHCP_IsServerDetected Function

## C

    bool TCPIP_DHCP_IsServerDetected(
        TCPIP_NET_HANDLE hNet
    );

## Description

This function determines if the DHCP client on the specified interface received any reply from a DHCP server.

## Preconditions

The DHCP module must be initialized.

## Parameters

Parameters | Description
--- | ---
hNet | Interface to query.

## Returns

- True - At least one DHCP server is attached to the specified network interface.
- False - No DHCP servers are currently detected on the specified network interface.

## Remarks

None.