Jump to main content

##

# DRV_ENCX24J600_Reinitialize Function

## C

    void DRV_ENCX24J600_Reinitialize(SYS_MODULE_OBJ object, const SYS_MODULE_INIT * const init);

## Returns

None

## Description

ENCX24J600 Reinitialization This function will deinitialize and initialize the driver instance. As with DRV_ENCX24J600_Initialize DRV_ENCX24J600_SetMacCtrlInfo must be called for the driver to be useful.

## Remarks

This function is not planned to be implemented for the first release.

## Preconditions

The driver had to be successfully initialized with DRV_ENCX24J600_Initialize.