Jump to main content

##

# IPV6_ULA_RESULT Enumeration

## C

    typedef enum {
    IPV6_ULA_RES_OK,
    IPV6_ULA_RES_BUSY = -1,
    IPV6_ULA_RES_IF_ERR = -2,
    IPV6_ULA_RES_NTP_ACCESS_ERR = -3,
    IPV6_ULA_RES_NTP_TSTAMP_ERR = -4
    } IPV6_ULA_RESULT;

## Description

Enumeration: IPV6_ULA_RESULT.

This enumeration provides a list of possible results for the Unique Local Address (ULA) generation.

## Members

Members | Description
--- | ---
IPV6_ULA_RES_OK | The address generation was started successfully.
IPV6_ULA_RES_BUSY = -1 | Address generation module is busy.
IPV6_ULA_RES_IF_ERR = -2 | Interface non-existent.
IPV6_ULA_RES_NTP_ACCESS_ERR = -3 | NTP module could not be accessed.
IPV6_ULA_RES_NTP_TSTAMP_ERR = -4 | Wrong NTP time stamp received.

## Remarks

None.