Jump to main content

##

# DRV_GMAC_Reinitialize Function

## C

    void DRV_GMAC_Reinitialize(SYS_MODULE_OBJ object, const SYS_MODULE_INIT * const init);

## Returns

None.

## Description

This function supports re-initialization of the PIC32 Ethernet MAC (opposite of set up).

## Remarks

This function is not supported yet.

## Preconditions

DRV_GMAC_Initialize must have been called to set up the driver.