Jump to main content

##

# TCPIP_DHCPS_IsEnabled Function

## C

    bool TCPIP_DHCPS_IsEnabled(
        TCPIP_NET_HANDLE hNet
    );

## Description

This function returns the current state of the DHCP Server on the specified interface.

## Preconditions

The DHCP server module should have been initialized.

## Parameters

Parameters | Description
--- | ---
hNet | Interface handle to query.

## Returns

- True - If successful.
- False - If unsuccessful.

## Remarks

None.