Jump to main content

##

# TCPIP_DHCP_Enable Function

## C

    bool TCPIP_DHCP_Enable(
        TCPIP_NET_HANDLE hNet
    );

## Description

This function enables the DHCP client for the specified interface, if it is disabled. If it is already enabled, no action is taken.

## Preconditions

The DHCP module must be initialized.

## Parameters

Parameters | Description
--- | ---
hNet | Interface to enable the DHCP client on.

## Returns

- True - If successful.
- False - If unsuccessful.

## Remarks

None.