Jump to main content

##

# DRV_GMAC_ConfigGet Function

## C

    size_t DRV_GMAC_ConfigGet(DRV_HANDLE hMac, void* configBuff, size_t buffSize, size_t* pConfigSize);

## Returns

- number of bytes copied into the supplied storage buffer

## Description

This function will get the current MAC driver configuration and store it into a supplied buffer.

## Remarks

- None

## Preconditions

DRV_GMAC_Initialize() should have been called. DRV_GMAC_Open() should have been called to obtain a valid handle.