Jump to main content

##

# TCPIP_SNMPV3_USERDATABASECONFIG_TYPE Enumeration

## C

    typedef enum {
    SNMPV3_USERNAME_CONFIG_TYPE = 0,
    SNMPV3_AUTHPASSWD_CONFIG_TYPE,
    SNMPV3_PRIVPASSWD_CONFIG_TYPE,
    SNMPV3_AUTHPASSWDLOCALIZEDKEY_CONFIG_TYPE,
    SNMPV3_PRIVPASSWWDLOCALIZEDKEY_CONFIG_TYPE,
    SNMPV3_HASHTYPE_CONFIG_TYPE,
    SNMPV3_PRIVTYPE_CONFIG_TYPE,
    SNMPV3_TARGET_SECURITY_NAME_TYPE,
    SNMPV3_TARGET_SECURITY_LEVEL_TYPE,
    SNMPV3_TARGET_SECURITY_MODEL_TYPE,
    SNMPV3_TARGET_MP_MODEL_TYPE,
    SNMPV3_ENGINE_ID_TYPE,
    SNMPV3_ENGINE_BOOT_TYPE,
    SNMPV3_ENGINE_TIME_TYPE,
    SNMPV3_ENGINE_MAX_MSG_TYPE
    } TCPIP_SNMPV3_USERDATABASECONFIG_TYPE;

## Description

Enumeration: TCPIP_SNMPV3_USERDATABASECONFIG_TYPE.

These configuration types are used by the SNMP user while doing configuration SNMPv3 parameters. It includes SNMpv3 user name , authentication and encryption configuration parameters.

## Members

Members | Description
--- | ---
SNMPV3_USERNAME_CONFIG_TYPE = 0 | Snmpv3 user name configuration.
SNMPV3_AUTHPASSWD_CONFIG_TYPE | Authentication configuration type.
SNMPV3_PRIVPASSWD_CONFIG_TYPE | Encryption and Decryption password configuration.
SNMPV3_AUTHPASSWDLOCALIZEDKEY_CONFIG_TYPE | Authorization localized key configuration type.
SNMPV3_PRIVPASSWWDLOCALIZEDKEY_CONFIG_TYPE | Encryption and Decryption password localized key configuration type.
SNMPV3_HASHTYPE_CONFIG_TYPE | SNMPv3 hash algorithm type.
SNMPV3_PRIVTYPE_CONFIG_TYPE | SNMPv3 privacy configuration type.
SNMPV3_TARGET_SECURITY_NAME_TYPE | SNMPv3 target address user name . This is for Trap communication.
SNMPV3_TARGET_SECURITY_LEVEL_TYPE | SNMPv3 target security type.
SNMPV3_TARGET_SECURITY_MODEL_TYPE | SNMPv3 target security model type.
SNMPV3_TARGET_MP_MODEL_TYPE | SNMPv3 target security message processing model type.
SNMPV3_ENGINE_ID_TYPE | Identifier that uniquely and unambiguously identifies the local SNMPv3 engine.
SNMPV3_ENGINE_BOOT_TYPE | Number of times the local SNMPv3 engine has rebooted or reinitialized since the engine ID was last changed.
SNMPV3_ENGINE_TIME_TYPE | Number of seconds since the local SNMPv3 engine was last rebooted or reinitialized.
SNMPV3_ENGINE_MAX_MSG_TYPE | SNMPv3 Engine Maximum message size the sender can accommodate.

## Remarks

None.