Jump to main content

##

# TCPIP_DHCPS_LeaseEntryRemove Function

## C

    bool TCPIP_DHCPS_LeaseEntryRemove(
        TCPIP_NET_HANDLE netH,
        TCPIP_MAC_ADDR* hwAdd
    );

## Description

This function is used to remove one entry from the leased HASH table with respect to the interface and the MAC address.

## Preconditions

The DHCP server module should have been initialized.

## Parameters

Parameters | Description
--- | ---
netH | Interface handle to use.
hwAdd | MAC address that needs to be removed from the HASH table.

## Returns

- True - If successful. _ False If unsuccessful.

## Remarks

This function is called from the command line to remove one entry and from the Wi-FI Driver module to remove a node that is disconnected from the AP.