Jump to main content

##

# TCPIP_ARP_ENTRY_TYPE Enumeration

## C

    typedef enum {
    ARP_ENTRY_TYPE_INVALID,
    ARP_ENTRY_TYPE_PERMANENT,
    ARP_ENTRY_TYPE_COMPLETE,
    ARP_ENTRY_TYPE_INCOMPLETE,
    ARP_ENTRY_TYPE_ANY,
    ARP_ENTRY_TYPE_TOTAL
    } TCPIP_ARP_ENTRY_TYPE;

## Description

Enumeration: TCPIP_ARP_ENTRY_TYPE.

List of different ARP cache entries.

## Members

Members | Description
--- | ---
ARP_ENTRY_TYPE_INVALID | Empty entry.
ARP_ENTRY_TYPE_PERMANENT | Entry valid and permanent.
ARP_ENTRY_TYPE_COMPLETE | Entry valid.
ARP_ENTRY_TYPE_INCOMPLETE | Entry not resolved yet.
ARP_ENTRY_TYPE_ANY | Any busy entry (PERMANENT
ARP_ENTRY_TYPE_TOTAL | Total entries - the number of entries the cache can store.

## Remarks

None.