Jump to main content

##

# TCPIP_ICMP_ECHO_REQUEST_RESULT Enumeration

## C

    typedef enum {
        TCPIP_ICMP_ECHO_REQUEST_RES_OK = 0,
        TCPIP_ICMP_ECHO_REQUEST_RES_TMO = -1
    } TCPIP_ICMP_ECHO_REQUEST_RESULT;

## Description

A result code for an echo request callback (as a result of an ICMP TCPIP_ICMP_EchoRequest() call).

## Members

Members | Description
--- | ---
TCPIP_ICMP_ECHO_REQUEST_RES_OK = 0 | A reply has been successfully received error codes, < 0.
TCPIP_ICMP_ECHO_REQUEST_RES_TMO = -1 | No reply recceived. The current request time out and will be deleted.