Jump to main content

##

# 1.2.1.15.2 NetBIOS Name Service (NBNS) Configurations

NBNS Specific User Configurations

- NBNS Task Rate (in msec):
  - NBNS task processing rate, in milliseconds.
  - The NBNS module will process a timer event with this rate for maintaining its own queues, processing timeouts, etc.
  - The lower the rate (higher the frequency) the higher the module priority and higher module performance can be obtained
  - The value cannot be lower than the TCPIP_STACK_TICK_RATE.
  - Default value: 110
  - Symbol TCPIP_NBNS_TASK_TICK_RATE