Jump to main content

##

# 1.2.1.15.3 Library Interface

Name | Description
--- | ---
Macros |
TCPIP_NBNS_TASK_TICK_RATE | NBNS task processing rate The default value is 110 milliseconds. The lower the rate (higher the frequency) the higher the module priority and higher module performance can be obtained The value cannot be lower than the TCPIP_STACK_TICK_RATE.
Functions |
TCPIP_NBNS_Task | Standard TCP/IP stack module task function.
Data Types and Constants |
TCPIP_NBNS_MODULE_CONFIG | Placeholder for NBNS configuration upgrades.