Jump to main content

# 8.3 New Device Support

(Ask a Question)

## 8.3.1 PolarFire

(Ask a Question)

### 8.3.1.1 Production Timing and Power for MPFS095T/TS/TL/TLS

(Ask a Question)

Table 8-1 8-2 8-3.Production Timing and Power for MPFS095T/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPFS095T/TS | EXT, IND | -1 | 1.0V, 1.05V
MPFS095T/TS/TL/TLS | EXT, IND | STD | 1.0V, 1.05V

### 8.3.1.2 Production Timing and Power for MPFS160T/TS/TL/TLS

(Ask a Question)

Table 8-1 8-2 8-3.Production Timing and Power for MPFS160T/TS/TL/TLS
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPFS160T/TS | EXT, IND | -1 | 1.0V, 1.05V
MPFS160T/TS/TL/TLS | EXT, IND | STD | 1.0V, 1.05V

### 8.3.1.3 Production Timing for MPFS250TS MIL

(Ask a Question)

Table 8-1 8-2 8-3.Production Timing for MPFS250TS MIL
Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
MPFS250TS | MIL | STD | 1.0V, 1.05V

Rev: 2026.1

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.