Jump to main content

# 2.3 New Device Support

(Ask a Question)

## 2.3.1 PolarFire

(Ask a Question)

### 2.3.1.1 New PolarFire FPGA Core Devices

(Ask a Question)

Libero SoC v2025.1 introduces the following PolarFire core devices with programming support.

Device | Temp-range | Speed-grade | Voltage | Timing/Power
--- | --- | --- | --- | ---
MPF050TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPF100TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPF200TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPF300TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPF500TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production

### 2.3.1.2 New PolarFire FPGA TS Automotive TGrade2 Devices

(Ask a Question)

Libero SoC v2025.1 introduces the following PolarFire TS Automotive TGrade2 devices.

Device | Temp-range | Speed-grade | Voltage | Timing/Power
--- | --- | --- | --- | ---
MPF100TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production
MPF200TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production
MPF300TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production
MPF500TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production

## 2.3.2 PolarFire SoC

(Ask a Question)

### 2.3.2.1 New PolarFire SoC Core Devices

(Ask a Question)

Libero SoC v2025.1 introduces the following PolarFire SoC core devices with programming support.

Device | Temp-range | Speed-grade | Voltage | Timing/Power
--- | --- | --- | --- | ---
MPFS025TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPFS095TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPFS160TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPFS250TC | EXT, IND, TGrade2 | STD | 1.0V, 1.05V | Production
MPFS460TC | EXT, IND | STD | 1.0V, 1.05V | Production

### 2.3.2.2 New PolarFire SoC TS Automotive TGrade2 Devices

(Ask a Question)

Libero SoC v2025.1 introduces the following PolarFire SoC TS Automotive TGrade2 devices.

Device | Temp-range | Speed-grade | Voltage | Timing/Power
--- | --- | --- | --- | ---
MPFS025TS | TGrade2 | STD | 1.0V, 1.05V | Production
MPFS095TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production
MPFS160TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production
MPFS250TS | TGrade2 | STD, -1 | 1.0V, 1.05V | Production

### 2.3.2.3 Military Production Timing and Power

(Ask a Question)

In the Libero SoC v2025.1 release, the following Military temperature range device achieves production timing and power.

Device | Temp-range | Speed-grade | Voltage | Timing/Power
--- | --- | --- | --- | ---
MPFS460TS | MIL | STD | 1.0V, 1.05V | Production

## 2.3.3 RT PolarFire

(Ask a Question)

- The Libero SoC v2025.1 release introduces a new FC1509 package for RTPF500ZT/ZTS/ZTL/ZTLS devices.
- SSN analysis is added for CG1509 package for RTPF500ZT/TS/TL/TLS and RTPF500T/TS/TL/TLS devices.

## 2.3.4 RT PolarFire SoC

(Ask a Question)

- Libero SoC v2025.1 introduces a new FC1509 package for RTPFS460ZT/ZTS/ZTL/ZTLS devices.
- Programming and SmartDebug support have been added for RTPFS460ZT/ZTS/ZTL/ZTLS and RTPFS160ZT/TS/TL/TLS devices.
- PFSOC_SCSM: SC_WAKE control is enabled by dynamic signals from fabric logic to allow temporary exit from System Controller Suspend mode to perform System Services.

Rev: 2025.2

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.