Jump to main content

# 9.3 New Device Support

(Ask a Question)

## 9.3.1 RT PolarFire

(Ask a Question)

### 9.3.1.1 Production Timing and Power

(Ask a Question)

Device | Temp-range | Speed-grade | Voltage
--- | --- | --- | ---
RTPF500T/TS | MIL | -1 | 1.0V, 1.05V
RTPF500T/TS/TL/TLS | MIL | STD | 1.0V, 1.05V

In addition, Libero SoC v2022.1 inserts a new Analysis operating conditions option in the Project settings dialog to specify the Total Ionizing Dose (TID) radiation to be 100 krad for RT PolarFire designs.

## 9.3.2 PolarFire SoC

(Ask a Question)

### 9.3.2.1 Production Timing and Power for MPFS250T/TS/TL/TLS

(Ask a Question)

Device | Temperature Range | Speed Grade | Voltage
MPFS250T/TL | EXT | STD | 1.0V, 1.05V
MPFS250T/TL/TS/TLS | IND | STD | 1.0V, 1.05V
MPFS250T | EXT | -1 | 1.0V, 1.05V
MPFS250T/TS | IND | -1 | 1.0V, 1.05V

### 9.3.2.2 Production Timing and Power for MPFS025T/TS/TL/TLS

(Ask a Question)

Device | Temperature Range | Speed Grade | Voltage
MPFS025T/TL | EXT | STD | 1.0V, 1.05V
MPFS025T/TL/TS/TLS | IND | STD | 1.0V, 1.05V
MPFS025T | EXT | -1 | 1.0V, 1.05V
MPFS025T/TS | IND | -1 | 1.0V, 1.05V

### 9.3.2.3 MPFS025T/TS/TL/TLS Packages

(Ask a Question)

Libero SoC v2022.1 introduces the following production packages, which replace the corresponding EVAL packages for the MPFS025T/TS/TL/TLS devices.

- FCVG484 replaces FCVG484_EVAL.
- FCSG325 replaces FCSG325_EVAL.

Note: The conversion is automatic if you open an existing design containing the EVAL package. However, user Tcl scripts must be changed to use the new package names.

## 9.3.3 Programming and SmartDebug

(Ask a Question)

Libero SoC v2022.1 introduces:

- Programming support for the MPFS160T/TS/TL/TLS PolarFire SoC devices.
- Programming and SmartDebug support for the MPF050T/TS/TL/TLS PolarFire devices.

## 9.3.4 SmartFusion2 and IGLOO2

(Ask a Question)

### 9.3.4.1 New 784 VFG Package for M2S060T/TS and M2GL060T/TS Devices

(Ask a Question)

Family | Device | Package | Speed | Platinum | Gold | Evaluation | Silver
SmartFusion2 | M2S060T/TS | VFG784 | -1, STD | yes | yes | yes | no
IGLOO2 | M2GL060T/TS | VFG784 | -1, STD | yes | yes | yes | no

## 9.3.5 PolarFire

(Ask a Question)

### 9.3.5.1 MPF300TS_ES Device Licenses

(Ask a Question)

The Silver license now supports the following PolarFire Kit-based MPF300TS_ES devices.

Device | Package | Speed Grade | Temperature Range
MPF300TS_ES | FCG484 | -1, STD | EXT, IND
MPF300TS_ES | FCG1152 | -1 | EXT, IND

Rev: 2025.2

The online versions of the documents are provided as a courtesy. Verify all content and data in the device’s PDF documentation found on the device product page.