Jump to main content

##

# 3.3 Wifi Provisioning via WPS

This example compiles the Wifi Provisioning via WPS application which is used to provision a WiFi connection.

## Description

In this demonstration, the WINC Driver will move into WPS mode – PIN or PBC. By activating the WPS mode in the AP concurrently, a WiFi connection is established.

## Downloading and building the application

To download or clone this application from Github, go to the top level of the repository

Path of the application within the repository is apps/wifi_provisioning_via_wps/firmware .

To build the application, refer to the following table and open the project using its IDE.

Project Name | Description
--- | ---
sam_d21_xpro_winc1500.X | MPLABX project for SAMD21 and WINC1500 Xplained pro
sam_e54_xpro_winc1500.X | MPLABX project for SAME54 and WINC1500 Xplained pro

## Setting up SAMXXX Xplained Pro board

- Connect the Debug USB port on the SAMXXX Xplained Pro board to the computer using a micro USB cable

## Running the Application

1. Open the project.
2. Build and program the generated code into the hardware using its IDE.
3. Please refer "WINC Firmware Update Guide" and "WINC Driver Demonstrations" for more information.