Jump to main content

##

# 1.3.1.4.10 EMU_EEPROM_STATUS Enum

## C

    typedef enum
    {
        /* Operation is successful or EEPROM Emulator is successfully initialized. */
        EMU_EEPROM_STATUS_OK,
        /* No EEPROM section has been allocated in the device */
        EMU_EEPROM_STATUS_ERR_NO_MEMORY,
        /* If an address outside the valid emulated EEPROM memory space was supplied */
        EMU_EEPROM_STATUS_ERR_BAD_ADDRESS,
        /* Emulated EEPROM memory is corrupt or not formatted or is incompatible with this version or scheme of the EEPROM emulator*/
        EMU_EEPROM_STATUS_ERR_BAD_FORMAT,
        /* Emulated EEPROM is not initialized */
        EMU_EEPROM_STATUS_ERR_NOT_INITIALIZED

    }EMU_EEPROM_STATUS;

## Summary

Identifies the current status/state of EEPROM operation.

## Description

This enumeration identifies the current status/state of the EEPROM operation

## Remarks

None