Jump to main content

##

# 1.2.1.5 SYS_MEDIA_PROPERTY Enum

## C

    typedef enum
    {
        /* Media supports Byte Write */
        SYS_MEDIA_SUPPORTS_BYTE_WRITES = 0x01,

        /* Media supports only Read operation */
        SYS_MEDIA_SUPPORTS_READ_ONLY = 0x02,

        /* Media supports OTP (One Time Programming) */
        SYS_MEDIA_SUPPORTS_ONE_TIME_PROGRAMING = 0x04,

        /* Read in blocking */
        SYS_MEDIA_READ_IS_BLOCKING = 0x08,

        /* Write is blocking */
        SYS_MEDIA_WRITE_IS_BLOCKING = 0x10,

    } SYS_MEDIA_PROPERTY;

## Summary

Contains information of property of a media.

## Description

This structure contains the information of property of a media device.

## Remarks

For a device, if multiple properties are applicable, they can be ORed together and used.