Jump to main content

##

# DRV_MX25L_GEOMETRY Struct

## C

    typedef struct
    {
        uint32_t read_blockSize;
        uint32_t read_numBlocks;
        uint32_t numReadRegions;

        uint32_t write_blockSize;
        uint32_t write_numBlocks;
        uint32_t numWriteRegions;

        uint32_t erase_blockSize;
        uint32_t erase_numBlocks;
        uint32_t numEraseRegions;

        uint32_t blockStartAddress;
    } DRV_MX25L_GEOMETRY;

## Summary

MX25L Device Geometry data.

## Description

This data type will be used to get the geometry details of the MX25L flash device.

## Remarks

None.