Jump to main content

##

# 1.1.4.4.19 DRV_NAND_FLASH_TRANSFER_STATUS Enum

## C

    typedef enum
    {
        /* Transfer is being processed */
        DRV_NAND_FLASH_TRANSFER_BUSY,

        /* Transfer is successfully completed */
        DRV_NAND_FLASH_TRANSFER_COMPLETED,

        /* Transfer is failed from NAND Flash */
        DRV_NAND_FLASH_TRANSFER_FAIL,

        /* Transfer had unknown error */
        DRV_NAND_FLASH_TRANSFER_ERROR_UNKNOWN,
    } DRV_NAND_FLASH_TRANSFER_STATUS;

## Summary

NAND FLASH Driver Transfer Status

## Description

This data type will be used to indicate the current transfer status for NAND FLASH driver.

## Remarks

None.