Jump to main content

##

# 1.3.1.4.9 EMU_EEPROM_BufferRead Function

## C

    EMU_EEPROM_STATUS EMU_EEPROM_BufferRead(
        const uint16_t offset,
        uint8_t *const data,
        const uint16_t length
    );

## Summary

Reads a buffer of data from the emulated EEPROM memory space

## Description

Reads a buffer of data from a section of emulated EEPROM memory space. The destination buffer may be of any size, and the source may lie outside of an emulated EEPROM page boundary.

## Precondition

Function EMU_EEPROM_Initialize should have been called before calling this function.

## Parameters

Param | Description
--- | ---
offset | Starting byte offset to read from, in emulated EEPROM memory space
data | Pointer to the destination data buffer to fill
length | Length of the data to read, in bytes

## Returns

EMU_EEPROM_STATUS - Enum of type EMU_EEPROM_STATUS. Status code indicating the status of the operation.

## Example

    uint8_t my_buffer[5];

    EMU_EEPROM_BufferRead(0, my_buffer, 5);

## Remarks

None }