Jump to main content

##

# 1.2.6.11 SYS_DMA_WIDTH Enum

## C

    typedef enum
    {
        /* DMA data width 8 bit */
        SYS_DMA_WIDTH_8_BIT,

        /* DMA data width 16 bit */
        SYS_DMA_WIDTH_16_BIT,

        /* DMA data width 32 bit */
        SYS_DMA_WIDTH_32_BIT,

        /* USed when DMA Width is not supported */
        SYS_DMA_WIDTH_NONE = -1

    }SYS_DMA_WIDTH;

## Summary

Enumeration of possible DMA data width

## Description

This data type provides an enumeration of all possible DMA data width.

## Remarks

Some of the enum elements may not be applicable for particular device, check MCC generated code before using them.