Jump to main content

##

# DRV_AT24_TRANSFER_STATUS Enum

## C

    typedef enum
    {
        /* Transfer is being processed */
        DRV_AT24_TRANSFER_STATUS_BUSY,

        /* Transfer is successfully completed */
        DRV_AT24_TRANSFER_STATUS_COMPLETED,

        /* Transfer had error */
        DRV_AT24_TRANSFER_STATUS_ERROR

    } DRV_AT24_TRANSFER_STATUS;

## Summary

Defines the data type for AT24 Driver transfer status.

## Description

This will be used to indicate the current transfer status of the AT24 EEPROM driver operations.

## Remarks

None.