Jump to main content

##

# 2.6.4.6 USB_DEVICE_HID_EVENT_DATA_GET_IDLE Structure

## C

    typedef struct {
      uint8_t reportID;
    } USB_DEVICE_HID_EVENT_DATA_GET_IDLE;

## Summary

USB Device HID Get Idle Event Data

This defines the data type of the data generated to the HID event handler on a USB_DEVICE_HID_EVENT_GET_IDLE event.

## Members

Members | Description
uint8_t reportID; | The protocol code

## Remarks

None.