Jump to main content

##

# 3.3.3.1 USB_HOST_AUDIO_V1_ATTACH_LISTENERS_NUMBER Macro

## C

    #define USB_HOST_AUDIO_V1_ATTACH_LISTENERS_NUMBER

## Summary

USB Host Audio v1.0 Attach Listeners Number

The USB Audio v1.0 Host Client Driver provides attach notification to listeners who have registered with the client driver via the USB_HOST_AUDIO_V1_0_AttachEventHandlerSet() function. The USB_HOST_AUDIO_V1_0_ATTACH_LISTENERS_NUMBER configuration constant defines the maximum number of event handlers that can be set. This number should be set to equal the number of entities that interested in knowing when a Audio v1.0 device is attached.

## Remarks

None.