Jump to main content

##

# 2.6.3 Configuring the Library

The following configuration parameters must be defined while using the HID Function Driver. The configuration macros that implement these parameters must be located in the `system_config.h` file in the application project and a compiler include path (to point to the folder that contains this file) should be specified.

## Macros

Name | Description
USB_DEVICE_HID_INSTANCES_NUMBER | Specifies the number of HID instances
USB_DEVICE_HID_QUEUE_DEPTH_COMINED | DOM-IGONORE-BEGIN
Configuration on MCC | This section describes the symbols available in the MCC that can be configured