Jump to main content

##

# 2.2.4.48 USB_DEVICE_EVENT_DATA_CONFIGURED Structure

## C

    typedef struct {
      uint8_t configurationValue;
    } USB_DEVICE_EVENT_DATA_CONFIGURED;

## Summary

USB Device Set Configuration Event Data type.

This data type defines the type of data that is returned by the Device Layer along with the USB_DEVICE_EVENT_CONFIGURED event.

## Members

Members | Description
uint8_t configurationValue; | The configuration that was set

## Remarks

None.