Jump to main content

##

# 3.2.4.19 USB_HOST_EVENT_RESPONSE Enumeration

## C

    typedef enum {
      USB_HOST_EVENT_RESPONSE_NONE = 0
    } USB_HOST_EVENT_RESPONSE;

## Summary

Host Layer Events Handler Function Response Type.

This is the definition of the Host Layer Event Handler Response Type.

## Members

Members | Description
USB_HOST_EVENT_RESPONSE_NONE = 0 | Returning this value indicates no application response to the host event.

## Remarks

None.