Jump to main content

##

# 2.6.4.10 USB_DEVICE_HID_EVENT_DATA_SET_IDLE Structure

## C

    typedef struct {
      uint8_t duration;
      uint8_t reportID;
    } USB_DEVICE_HID_EVENT_DATA_SET_IDLE;

## Summary

USB Device HID Set Idle Event Data Type.

This defines the data type of the data generated to the HID event handler on a USB_DEVICE_HID_EVENT_SET_IDLE event.

## Members

Members | Description
uint8_t duration; | Idle duration
uint8_t reportID; | Report ID

## Remarks

None.