Jump to main content

##

# 3.3.4.19 USB_HOST_AUDIO_V1_TerminalAssociationGet Function

## C

    uint8_t USB_HOST_AUDIO_V1_TerminalAssociationGet(
        USB_HOST_AUDIO_V1_OBJ audioObj,
        USB_HOST_AUDIO_V1_CONTROL_ENTITY_OBJ entityObject
    );

## Summary

This function returns the ID of the associated terminal type of the audio control terminal. Prior to calling this function the entity object should be obtained by calling USB_HOST_AUDIO_V1_ControlEntityGetFirst, USB_HOST_AUDIO_V1_ControlEntityGetNext, or USB_HOST_AUDIO_V1_EntityObjectGet.

## Parameters

Parameters | Description
audioObj | USB Host Audio v1.0 Device object
entityObject | Audio control entity object

## Returns

The ID of the associated terminal.