Jump to main content

##

# 2.5.4.9 USB_DEVICE_CDC_EVENT_DATA_SEND_BREAK Structure

## C

    typedef struct {
      uint16_t breakDuration;
    } USB_DEVICE_CDC_EVENT_DATA_SEND_BREAK;

## Summary

USB Device CDC Function Driver Send Break Event Data

This data type defines the data structure returned by the driver along with USB_DEVICE_CDC_EVENT_SEND_BREAK event.

## Members

Members | Description
uint16_t breakDuration; | Duration of break signal