Jump to main content

##

# 3.3.4.57 USB_HOST_AUDIO_V1_STREAM_EVENT_READ_COMPLETE_DATA Structure

## C

    typedef struct {
      USB_HOST_AUDIO_V1_STREAM_TRANSFER_HANDLE transferHandle;
      size_t length;
      USB_HOST_AUDIO_V1_RESULT result;
    } USB_HOST_AUDIO_V1_STREAM_EVENT_READ_COMPLETE_DATA, USB_HOST_AUDIO_V1_STREAM_EVENT_WRITE_COMPLETE_DATA;

## Summary

USB Host Audio v1.0 Class Stream Data Transfer Event Data.

This data type defines the data structure returned by the Audio V1.0 stream in conjunction with the following events:

- USB_HOST_AUDIO_V1_STREAM_EVENT_READ_COMPLETE_DATA
- USB_HOST_AUDIO_V1_STREAM_EVENT_WRITE_COMPLETE_DATA

## Members

Members | Description
USB_HOST_AUDIO_V1_STREAM_TRANSFER_HANDLE transferHandle; | Transfer handle of this transfer
size_t length; | Amount of data transferred
USB_HOST_AUDIO_V1_RESULT result; | Transfer termination status

## Remarks

None.